; CCLfish control file 805WR.CCL
; Copyright 1998, by the University of California. 
; Unauthorized commercial use is prohibited. 

Title
Sample problems for tuning coupled-cavity linac cells.
Resonant frequency = 805 MHz, Bore radius = 2.25 cm
ENDTitle
 
PARTICLE              H+
 
FILEname_prefix       805WR
SEQuence_number       1
PI_MODE
FREQuency             805
BETA                  0.4350009365479
LENGTH                8.1
DIAMeter              28.365
G_OVER_Beta_lambda    0.2424933584088
GAP_Length            3.928392406223
E0_Normalization      1.5
E0T_Normalization     1.211078158199
;EQUATOR_Flat         0.576 ; for use in CDTFISH
OUTER_CORNer_radius   3
INNER_CORNer_radius   0.5
INNER_NOSE_radius     0.085
OUTER_NOSE_radius     0.25
FLAT_length           0
CONE_angle            20
SEPTUM_thickness      1.524
BORE_radius           2.25
PHASE_length          90
Ring_Type             4
RING_DY               0
RING_Effect           4
RING_Width            2.50
RING_Angle            45
RING_Thickness        0.1927
DELTA_frequency       0.02
MESH_size             0.035
INCrement             2
START                 4

; Start codes for CCLFISH:
; 1 No tuning
; 2 Adjust diameter
; 3 Adjust spectum thickness (not recommended)
; 4 Adjust gap
; 5 Adjust cone angle

ENDFile

